# One Compartment Model with Absorption estimating KA and CL

[Generated automatically as a Tutorial summary]

## Inputs

### Description

Name: | dep_one_cmp_ka_cl_stderr
Title: | One Compartment Model with Absorption estimating KA and CL
Author: | Wright Dose Ltd
Abstract: |

One Compartment Model with Absorption compartment with rate (KA).
Elimination rate parametrised by clearance (CL)
and volume of distribution (V).
Model specification uses incremental flows

Keywords: | dep_one_cmp_cl; one compartment model
Input Script: | `dep_one_cmp_ka_cl_stderr.pyml`
Diagram: |

Failed to create compartment diagram

### True f[X] values

    f[KA] = 0.3
    f[V] = 20
    f[CL] = 3

### Starting f[X] values

    f[KA] = 0.3
    f[V] = 18.003
    f[CL] = 3

## Outputs

### Generating and Fitting Summaries

- Gen: One Compartment Model with Absorption estimating KA and CL (gen)
- Fit: One Compartment Model with Absorption estimating KA and CL (fit)

### Fitted f[X] values

    f[KA] = 0.27392
    f[V] = 18.003
    f[CL] = 3.2389

## Plots

### Dense comp plots

Alternatively see All dense_comp graph plots

## Comparison

### True objective value

    -42.0983665907

### Final fitted objective value

    -44.7677718765

### Compare Main f[X]

Name | Initial | Fitted | True | Prop. Error | Abs. Error
--- | --- | --- | --- | --- | ---
f[KA] | 0.3 | 0.274 | 0.3 | 8.69% | 2.61e-02
f[CL] | 3 | 3.24 | 3 | 7.96% | 2.39e-01

### Compare Noise f[X]

No Noise f[X] values to compare.

### Compare Variance f[X]

No Variance f[X] values to compare.