# One Compartment Model with Absorption estimating V and CL

[Generated automatically as a Generation summary]

## Inputs

### Description

Name: | d1cmp_v_cl_stderr
Title: | One Compartment Model with Absorption estimating V and CL
Author: | Wright Dose Ltd
Abstract: |

One Compartment Model with Absorption compartment with rate (KA).
Elimination rate parametrised by clearance (CL)
and volume of distribution (V).
Model specification uses incremental flows

Keywords: | dep_one_cmp_cl; one compartment model
Input Script: | `d1cmp_v_cl_stderr_gen.pyml`
Diagram: |

### True f[X] values

    f[KA] = 0.3000
    f[V] = 20.0000
    f[CL] = 3.0000

## Outputs

### Generated parameter .csv files

Fixed Effects: | `fx_params.csv (gen)`
Random Effects: | `rx_params.csv (gen)`
Model params: | `mx_params.csv (gen)`
State values: | `sx_params.csv (gen)`
Predictions: | `px_params.csv (gen)`
Synthetic Data: | `synthetic_data.csv (gen)`

## Plots

### Dense sim plots

Alternatively see All dense_sim graph plots